Quantum Dot Molecules as Spin-Photon Interfaces for Applications in Quantum Communication

L. Hanschke4, C. Thalacker1, M. Lienhart1, F. Bopp1, F. Vögl1, N. Bart2, J. Schall3, K. Boos4, F. Sbresny4, M. Stöcker1, A. Wieck2, A. Ludwig2, D. Reuter5, S. Reitzenstein3, H.Riedl1, K. Müller4 and J. J. Finley1

1Walter Schottky Institute, TUM School of Natural Sciences, Technical University of Munich, Garching bei München, Germany

2Faculty of Physics and Astronomy, Ruhr-University Bochum, Bochum, Germany

3Institute of Solid-State Physics, Technical University of Berlin, Berlin, Germany

4Walter Schottky Institute, TUM School of Computation, Information, and Technology, Technical University of Munich, Garching bei München, Germany

5University of Paderborn, Paderborn, Germany

Long coherence times, strong light-matter coupling, and tunability lie at the heart of all hardware for distributed quantum information technologies. Spin-photon interfaces based on III-V semiconductor quantum dots (QDs) are a promising platform for such technologies since they combine properties such as light-matter-interactions, robust spin-photon selection rules, dominant emission into the zero-phonon line at low temperatures, and ease of integration into opto-electronic devices. Together, these properties make QDs promising as spin-photon interfaces. Tunnel-coupled pairs of QDs, so called QD-molecules (QDMs), additionally exhibit enhanced coherence times (T2\*) using two-spin singlet-triplet (S-T0) qubits [1] which are inherently protected against electric and magnetic field noise.

To unlock the increased coherence times of QDMs, we developed and investigated a device, where a single QDM is embedded in a low capacitance p-i-n diode structure (diode area: 10 µm x 25 µm) that allows for fast electrical switching (>500 MHz) and thus fast control of the tunnel coupling. A circular Bragg grating is deterministically positioned via in-situ electron beam lithography on top of a single QDM. In combination with a distributed Bragg reflector below the QDM, we achieve photon extraction efficiencies of up to 24.4% [2].

Additionally, we demonstrated sequential and all-optical charging of the QDM via tunneling ionization. We show one- and two-hole charging efficiencies of (93.5 ± 0.8)% and (80.5 ± 1.3)%, respectively [3]. Combining the control of the charge state, precise setting and fast switching of the inter-dot coupling, and high photon extraction efficiencies provides a perspective to use our devices for the deterministic generation of one- and two-dimensional photonic cluster states [4].

[1] S. G. Carter et al., Coherent population trapping combined with cycling transitions for quantum dot hole spins using triplet trion states, Phys. Rev. Lett. 126, 107401 (2021).

[2] J. Schall et al., Bright electrically controllable quantum-dot-molecule devices fabricated by in situ electron-beam lithography, Adv. Quantum Technol., 4, 6, (2021).

[3] F. Bopp et al., Quantum dot molecule devices with optical control of charge status and electronic control of coupling, Adv. Quantum Technol., 5, 2200049 (2022).

[4] S. E. Economou et al., Optically generated 2-dimensional photonic cluster state from coupled quantum dots, Phys. Rev. Lett. 105, 093601 (2010).